|  |  |  |
| --- | --- | --- |
| **A. Product Information** | | |
| 01 | Tag/ID |  |
| 02 | CRRC Product ID Number |  |
| 03 | Manufacturer |  |
| 04 | Brand |  |
| 05 | Model |  |
| 06 | Product Type |  |
| 07 | Roof Pitch |  |

|  |  |  |
| --- | --- | --- |
| **B. SRI Calculations** | | |
| 01 | Is Aged Reflectance Listed with CRRC? (Yes or No) |  |
| 02 | CRRC Listed Aged Solar Reflectance |  |
| 03 | Initial Solar Reflectance |  |
| 04 | Calculated Aged Solar Reflectance |  |
| 05 | Thermal Emittance |  |

|  |  |  |
| --- | --- | --- |
| **C. Results** | | |
| 01 | Solar Reflectance Index |  |

|  |  |
| --- | --- |
| **Documentation Author's Declaration Statement** | |
| 1. I certify that this Certificate of Compliance documentation is accurate and complete. | |
| Documentation Author Name: | Documentation Author Signature: |
| Company: | Signature Date: |
| Address: | CEA/ HERS Certification Identification (if applicable): |
| City/State/Zip: | Phone: |
| **Responsible Person's Declaration statement** | |
| I certify the following under penalty of perjury, under the laws of the State of California:   1. The information provided on this Certificate of Compliance is true and correct. 2. I am eligible under Division 3 of the Business and Professions Code to accept responsibility for the building design or system design identified on this Certificate of Compliance (responsible designer). 3. That the energy features and performance specifications, materials, components, and manufactured devices for the building design or system design identified on this Certificate of Compliance conform to the requirements of Title 24, Part 1 and Part 6 of the California Code of Regulations. 4. The building design features or system design features identified on this Certificate of Compliance are consistent with the information provided on other applicable compliance documents, worksheets, calculations, plans and specifications submitted to the enforcement agency for approval with this building permit application. 5. I will ensure that a registered copy of this Certificate of Compliance shall be made available with the building permit(s) issued for the building, and made available to the enforcement agency for all applicable inspections. I understand that a registered copy of this Certificate of Compliance is required to be included with the documentation the builder provides to the building owner at occupancy. | |
| Responsible Designer Name: | Responsible Designer Signature: |
| Company: | Date Signed: |
| Address: | License: |
| City/State/Zip: | Phone: |

**CF1R-ENV-04-E User Instructions**

Calculate the SRI value by using theSolar Reflectance Index (SRI) Calculation Worksheet found on the California Energy Commission website at: <http://energy.ca.gov/title24/2013standards/documents/solar_reflectance/>.

**A. Product Information**

1-6.Tag/ID, CRRC Product ID Number, Manufacturer, Brand, Model and Product Type should be based on product information from the Cool Roof Rating Council’s website. The product directory is located at <http://www.coolroofs.org/products/search.php> and may be browsed either by viewing all products or by using the search function to find a specific product. Keep in mind that inclusion in the directory does not guarantee that a product will meet the energy requirements.

7. Roof Pitch: Designate the roof slope as either “less than or equal to 2:12”(≤2:12) or “greater than 2:12”(>2:12). A ratio of 2:12 is approximately 9.5 degree slope. The SRI requirement is based partly on the slope of the roof.

**B. SRI Calculations**

1. Aged Reflectance Listed with CRRC?: Indicate whether or not your product’s 3-year Aged Solar Reflectance is listed on the CRRC website by selecting either “yes” or “no” from the drop-down list. Depending on your selection, the boxes that you will not need should become blacked out.
2. CRRC Listed Aged Solar Reflectance: If you selected “yes” to box 1, input the CRRC listed 3-year Aged Solar Reflectance.
3. Initial Solar Reflectance: If you selected “no” to box 1, input the CRRC listed Initial Solar Reflectance value as a decimal between 0 and 1.
4. Calculated Aged Solar Reflectance: No input required. The calculator will calculate the Aged Solar Reflectance using the Initial Solar Reflectance once you hit enter or click outside the box.
5. Thermal Emittance: Input the value for Thermal Emittance obtained from the CRRC. This value can be either the Initial Thermal Emittance or the 3-year aged value. Note that it also must be a decimal between 0 and 1.

**C. Results**

1. Solar Reflectance Index: If you have entered values for both Solar Reflectance and Thermal Emittance, once you press enter or click outside the box, the calculator will calculate the final SRI value. It may take a few moments to obtain a value for the SRI depending on the values you inputted for Reflectance and Emittance. Transfer the proposed SRI value to the “SRI (Optional)” column of the appropriate CF1R-NCB, -ADD, or -ALT certificate of compliance.

|  |  |  |
| --- | --- | --- |
| **A. Product Information** | | |
| 01 | Tag/ID | <<reference from CF1R>> |
| 02 | CRRC Product ID Number | << user input: text >> |
| 03 | Manufacturer | <<user input: text>> |
| 04 | Brand | <<user input: text>> |
| 05 | Model | <<user input: text>> |
| 06 | Product Type | <<text (data from CF-1R>> |
| 07 | Roof Pitch | <<text (data from CF-1R>> |

|  |  |  |
| --- | --- | --- |
| **B. SRI Calculation** | | |
| 01 | Is Aged Reflectance Listed with CRRC? (Yes or No) | <<user pick from list: Yes; No>> |
| 02 | CRRC Listed Aged Solar Reflectance | <<if B01 = Yes, then user input: numeric (x.xx, value must be > 0 and < 1); else display NA>> |
| 03 | Initial Solar Reflectance | <<if B01 = No, then user input: numeric (x.xx, value must be > 0 and < 1); else display NA>> |
| 04 | Calculated Aged Solar Reflectance | <<if B01 = No, then user input: numeric (x.xx, value must be > 0 and < 1); else display NA>> |
| 05 | Thermal Emittance | <<user input: numeric (x.xx, value must be > 0 and < 1)>> |

|  |  |  |
| --- | --- | --- |
| **C. Results** | | |
| 01 | Solar Reflectance Index | <<user input: numeric (xxx, value must be > 0 and <=100)>> |